

**One Touch Cleaning:**

The self-clean design freezes the surface with moisture in the air and removes the dirt in defrosting.



**Easy Installation**

**UPS Inverter**

**Features:**

|  |  |
| --- | --- |
| Power Input (W) | **320~2204** |
| Running Current (A) | **1.4~10.2** |
| Refrigerant | **R410a** |
| Air Circulation (m3/h) | **850** |

HSU-18HFCF/022WUSDC(W)

Smart Inverter